APH Digital Recording Device Operation Instructions

Note: Due to battery shelf life, you may have to replace the batteries in this electronic device when received.

This device is APH Catalog Number 6-77505-01.

# Product Description

Small, oval handheld recording device

Front: A half-circle flat push-button for recording and playing is located near the top of the device. A small, red LED light is above and to the right of the button. A speaker is in the bottom half of the device. An oval, flat, ridged slide switch is on the top left of the device to toggle between Record (bottom switch setting) and Play (top switch setting).

Back: A circular battery compartment is in the middle of the device. This compartment has a coin-sized indentation in its center so that it can be turned counter-clockwise to open the battery compartment. There is a CE sticker, a WEEE (Waste Electrical and Electronic Equipment) Directive compliance sticker, and a “MADE IN CHINA” sticker.

# Operation

**PLAY/REC** slide switch: To play and record message

**Push-Button**: To activate recording and play

## Recording a Message

1. Slide the **PLAY/REC** to **“REC”** position.
2. Depress and hold the **push-button**, a lit LED indicating ready for recording, speak to the microphone (**MIC**) in a distance of 3 inches (7.6 cm). You can record up to 10 seconds message and the LED will be off at the end of 10 seconds. Release the **push-button** anytime when you finish your recording.
3. Slide the **PLAY/REC** switch to **“PLAY”** position. If you forget to do this, the recorded message will be erased when the **push-button** is depressed again.

## Playing the Message

1. Make sure the **PLAY/REC** switch is at **“PLAY”** position.
2. Press and release the push-button to hear the recorded message. You can stop playing the message anytime by pressing the **push-button** again during playing.

## Replacing an Existing Message

Simply follow the **“Recording a Message”** procedure as described above.

## Erasing the Message

Depress and release the **push-button** to erase the recorded message.

# Changing Batteries

A distorted sound during playback indicates the need for new batteries. To replace the battery, open the back cover, remove the old batteries (RE8822/RE8832: 2 x AG13, RE8869: 1 x CR2025) into the battery compartment with the positive (+) polarity facing the coil battery contact.

# Cautions:

Use only fresh batteries of the required size and type.

Never mix fresh batteries with old ones.